Connecting to 127.0.0.1:8991 (CONTROL)...  connected OK
Connecting to 127.0.0.1:8992 (DATA)...  connected OK
PID file timestamp: 20120831_143514
Server status:
  USB Running
  TM read thread running
  TM frames received: 49082
  TM frames invalid: 0

>StopUSB: Result: USB Stopped

>StartUSB: Result: USB Running

>XPO_RESET_ANALYZER = 0
Waiting for 100ms
XPO_RESET_ANALYZER = 1

>GPS: SiRF message 41:
 NAV: 0000 : 4 or more SV KF solution (GPS lock confirmed)
 TIME: 1703:484507897 = 2012-08-31 14:35:15.000
 POS: 43.935347 5.478835  65537 ASL
 SATS: 70320036 2 3 5 6 18 21 22 29 30 31   used 9

>Sending 139 byte command
TIMEOUT! Only 45 bytes sent

>XPStart: Started OK at 2012-08-31 14:35:18.0000 :: GPS sats: 4 or more
>Sleeping for 390000ms ...done.

>EOHO: End of orbit at 2012-08-31 14:41:49.0000 :: GPS sats: 4 or more
>Got 8570 new packets...
Got 8505 new packets...
Got 8285 new packets...
Got 8554 new packets...
Got 8303 new packets...
Got 5641 new packets...
Done! No new data received

>XPStop: 1

>Shutting down data thread... recv failed! result: -1
*** DATA READ THREAD TERMINATED ***
done.
