Connecting to 127.0.0.1:8991 (CONTROL)...  connected OK
Connecting to 127.0.0.1:8992 (DATA)...  connected OK
PID file timestamp: 20120831_170404
Server status:
  USB Running
  TM read thread running
  TM frames received: 48878
  TM frames invalid: 0

>StopUSB: Result: USB Stopped

>StartUSB: Result: USB Running

>XPO_RESET_ANALYZER = 0
Waiting for 100ms
XPO_RESET_ANALYZER = 1

>GPS: SiRF message 41:
 NAV: 0000 : 4 or more SV KF solution (GPS lock confirmed)
 TIME: 1703:493420649 = 2012-08-31 17:04:04.000
 POS: 43.935347 5.478834  65711 ASL
 SATS: 80260026 2 3 6 18 19 22 32   used 9

>Sending 139 byte command
TIMEOUT! Only 45 bytes sent

>XPStart: Started OK at 2012-08-31 17:04:07.0000 :: GPS sats: 4 or more
>Sleeping for 390000ms ...done.

>EOHO: End of orbit at 2012-08-31 17:10:38.0000 :: GPS sats: 4 or more
>Got 8570 new packets...
Got 8286 new packets...
Got 8330 new packets...
Got 8562 new packets...
Got 8329 new packets...
Got 5343 new packets...
Done! No new data received

>XPStop: 1

>Shutting down data thread... recv failed! result: -1
*** DATA READ THREAD TERMINATED ***
done.
