Connecting to 127.0.0.1:8991 (CONTROL)...  connected OK
Connecting to 127.0.0.1:8992 (DATA)...  connected OK
PID file timestamp: 20120908_002023
Server status:
  USB Running
  TM read thread running
  TM frames received: 48938
  TM frames invalid: 0

>StopUSB: Result: USB Stopped

>StartUSB: Result: USB Running

>XPO_RESET_ANALYZER = 0
Waiting for 100ms
XPO_RESET_ANALYZER = 1

>GPS: SiRF message 41:
 NAV: 0000 : 4 or more SV KF solution (GPS lock confirmed)
 TIME: 1704:519635193 = 2012-09-08 00:20:24.000
 POS: 43.935347 5.478819  65687 ASL
 SATS: 004800D8 4 5 7 8 20 23   used 9

>Sending 139 byte command
TIMEOUT! Only 45 bytes sent

>XPStart: Started OK at 2012-09-08 00:20:27.0000 :: GPS sats: 4 or more
>Sleeping for 340000ms ...done.

>EOHO: End of orbit at 2012-09-08 00:26:08.0000 :: GPS sats: 4 or more
>Got 8057 new packets...
Got 7814 new packets...
Got 7815 new packets...
Got 8054 new packets...
Got 7804 new packets...
Got 7823 new packets...
Got 474 new packets...
Done! No new data received

>XPStop: 1

>Shutting down data thread... recv failed! result: -1
*** DATA READ THREAD TERMINATED ***
done.
