Connecting to 127.0.0.1:8991 (CONTROL)...  connected OK
Connecting to 127.0.0.1:8992 (DATA)...  connected OK
PID file timestamp: 20120908_002737
Server status:
  USB Running
  TM read thread running
  TM frames received: 48938
  TM frames invalid: 0

>StopUSB: Result: USB Stopped

>StartUSB: Result: USB Running

>XPO_RESET_ANALYZER = 0
Waiting for 100ms
XPO_RESET_ANALYZER = 1

>GPS: SiRF message 41:
 NAV: 0000 : 4 or more SV KF solution (GPS lock confirmed)
 TIME: 1704:520028415 = 2012-09-08 00:27:37.000
 POS: 43.935353 5.478835  65697 ASL
 SATS: 004800DA 2 4 5 7 8 20 23   used 10

>Sending 139 byte command
TIMEOUT! Only 45 bytes sent

>XPStart: Started OK at 2012-09-08 00:27:40.0000 :: GPS sats: 4 or more
>Sleeping for 340000ms ...done.

>EOHO: End of orbit at 2012-09-08 00:33:21.0000 :: GPS sats: 4 or more
>Got 8052 new packets...
Got 8050 new packets...
Got 8053 new packets...
Got 8058 new packets...
Got 7777 new packets...
Got 7674 new packets...
Done! No new data received

>XPStop: 1

>Shutting down data thread... recv failed! result: -1
*** DATA READ THREAD TERMINATED ***
done.
